For 1990-2009 cars

### Fog Lamp Bulb Replacement

1. Reach up from underneath the front body panel, rotate the bulb socket counter-clockwise 1/4 of a turn while pressing the socket in firmly. Pull the socket rearward until the bulb clears the fog lamp housing.
2. Disconnect the wire connector from the bulb by lifting the lock tab and pulling it away from the plastic base.
3. Remove the bulb assembly and replace it with the appropriate bulb.

### Front Side Marker Lamp Replacement Bulb

1. Open the hood and secure it with the prop rod.
2. Release the pressure clip on the back of the marker lamp housing assembly. Pull the front leading edge of the marker lamp assembly out and forward.
3. Rotate the bulb socket counter-clockwise 1/4 of a turn. Pull the socket rearward until the bulb clears the marker lamp housing assembly.
4. Remove the bulb and replace it with the appropriate bulb.