For 1990-2009 cars

Use the following flow chart to determine if vehicle pull is most likely caused by steering pull or torque steer. Perform the road test on a flat level road and with minimum wind conditions.

Vehicle State | Performance Result
--- | ---
Drive -- Steady Speed: | 72-88 km/h (45-55 mph) in drive maintaining a steady speed
Neutral -- Coast: | 72-88 km/h (45-55 mph) in neutral Coasting