For 1990-2009 cars

### Removal Procedure

1. Remove the radio bezel trim plate.
2. Remove then radio-to-I/P screws.
3. Remove the radio electrical and antenna connectors and remove the radio.
4. Remove the control head-to-I/P screws.
5. Rotate the front of the control head upward and toward the front of vehicle to gain access to the bottom of the control head.
6. Remove the electrical connectors from the control head.
7. Rotate the temperature knob to the full hot position.
8. Rotate the control head downward and release the temperature cable flag by pushing the tab forward and pushing down on the cable at the same time.
9. Remove the temperature cable eyelet from the drive pin by squeezing the drive pin together.

### Installation Procedure

1. Rotate the temperature knob to the full hot position.
2. Install the cable eyelet onto the control head pin and install the cable housing flag into the slot in the control head until it engages the locking tab.
3. Install the electrical connectors to the control head.
4. Install the control head to I/P screws.

Tighten
Tighten the control head-to-I/P screws to 2.5 N·m (22 lb in).

5. Install the radio electrical and antenna connectors.
6. Install the radio to I/P screws.

Tighten
Tighten the I/P screws to radio to 2.5 N·m (22 lb in).

7. Install the radio trim bezel.