For 1990-2009 cars

## Cruise Control Cable Adjustment L61/L81

1. Partially disengage adjustment lock on cruise control throttle cable by depressing tabs (do not remove entirely). This will release spring inside adjuster to take out cable slack.

• | (1) - Cruise Control Throttle Cable

• | (2) - Adjuster (Shown here, actually further back on cable)

• | (3) - Cable Snap

• | (4) - Cable End

2. Make sure throttle plate is fully closed.
3. Ensure cable end is tight against cable snap.
4. Engage adjustment lock.