For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
O2 Sensor Clamp-to-Heat Shield | 4 N·m | 35 lb in
Back-Up Lamp Switch | 24 N·m | 18 lb ft
Ball Stud Into Steering Knuckle | 100 N·m | 75 lb ft
Battery Cable Terminals | 17 N·m | 13 lb ft
Battery Feed Cable-to-Underhood Fuse Block | 16 N·m | 12 lb ft
Battery Hold Down Bracket Fasteners | 20 N·m | 15 lb ft
Battery Tray Fasteners | 15 N·m | 11 lb ft
Console Front Fasteners | 2.5 N·m | 22 lb in
Console Rear Fasteners | 2.5 N·m | 22 lb in
Control Asm Rod-to-Control Lever Asm Pinch Bolt

- First Pass

12 N·m

9 lb ft

- Final Pass

180 degrees

Control Asm-to-Floor Pan Bolts | 8 N·m | 71 lb in
Control Shaft Lever Pivot Pin Bracket-to-Transaxle Bolts | 24 N·m | 18 lb ft
Differential Bearing Retainer-to-Transaxle Bolts | 24 N·m | 18 lb ft
Exhaust Manifold Pipe-to-Exhaust Manifold | 30 N·m | 25 lb ft
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Resonator | 20 N·m | 15 lb ft
Fluid Level Check and Fill Plug | 50 N·m | 37 lb ft
Frame-to-Body Bolts

- First Pass

90 N·m

60 lb ft

- Final Pass

45-60 degrees

Front Transaxle Mount Through Bolt | 55 N·m | 41 lb ft
Front Transaxle Mount-to-Transaxle | 55 N·m | 41 lb ft
Input Shaft Bearing Retainer Bolts | 38 N·m | 28 lb ft
Left Transaxle Mount Bolts | 55 N·m | 41 lb ft
Left Transaxle Mount Bracket-to-Transaxle Bolt | 55 N·m | 41 lb ft
Linkage Installer J 44015-to-Seat Tie Rod Ends | 45 N·m | 35 lb ft
Lower Control Arm Ball Stud Bolt and Nut-to-Steering Knuckle | 100 N·m | 75 lb ft
Output Shaft Bearing Retainer Bolts-Inner | 45 N·m | 33 lb ft
Output Shaft Bearing Retainer Bolts-Outer | 24 N·m | 18 lb ft
Rear Cover-to-Transaxle Bolts | 24 N·m | 18 lb ft
Rear Transaxle Mount Through Bolt | 90 N·m | 66 lb ft
Rear Transaxle Mount-to-Frame Bolts | 60 N·m | 44 lb ft
Rear Transaxle Mount-to-Transaxle | 55 N·m | 41 lb ft
Reverse Idler Gear Shaft Bolt | 24 N·m | 18 lb ft
Reverse Idler Gear Shaft Bracket Bolt | 24 N·m | 18 lb ft
Reverse Shift Lever Bolts | 24 N·m | 18 lb ft
Right Front Lower Splash Shield to Frame Assembly | 5 N·m | 44 lb in
Slave Cylinder Fasteners | 10 N·m | 7 lb ft
Stabilizer Bar Links-to-Strut Assemblies | 65 N·m | 50 lb ft
Steering Gear-to-Frame

- First Pass

45 N·m

35 lb ft

- Final Pass

90 degrees

Tie Rod End-to-Steering Knuckle | 60 N·m | 45 lb ft
Transaxle Case-to-Clutch Housing Bolts | 24 N·m | 18 lb ft
Transaxle Drain Plug | 50 N·m | 37 lb ft
Transaxle Fill Plug | 50 N·m | 37 lb ft
Transaxle Level Plug | 50 N·m | 37 lb ft
Transaxle Shift Control Shaft Block | 24 N·m | 18 lb ft
Transaxle-to-Engine Bolts | 65 N·m | 48 lb ft
Underhood Fuse Block Case Bolt | 9 N·m | 80 lb in
Wheel Bolts, Final Torque | 125 N·m | 92 lb ft
Wheel Bolts, Initial Torque | 63 N·m | 46 lb ft