For 1990-2009 cars

### Removal Procedure

1. Pull on the rear seat cushion retainer strap while pulling up on the cushion to disengage the seat cushion forward attachment.
2. Push the seat cushion rearward to disengage the attachment, then lift the cushion out of the vehicle.
3. Remove the seat cushion draw string and remove the seat cushion cover to expose the hog rings.
4. Remove the hog rings and remove the cover.

### Installation Procedure

1. Position the seat cushion cover over the seat cushion pad.
2. Install the hog rings to the seat cushion cover and to the cushion pad/frame.
3. Pull the draw string tight, and secure the draw string opening to the cushion frame.
4. Position the seat cushion over the floor area.
5. Route the seat belts through the cushion openings.
6. Slide the seat cushion frame into the attaching brackets.
7. Push downward on the forward retainers of the seat cushion to lock the cushion to the floor brackets.