For 1990-2009 cars

### EVAP Canister Check

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Caution: Refer to Relieving Fuel Pressure Caution in the Preface section.

An improperly functioning EVAP canister can cause problems with engine driveability and/or vehicle refueling. The canister can become plugged, with some internal obstruction or liquid fuel, or develop an air leak.

Stalling or poor driveability can be caused by a fuel saturated canister.

1. Disconnect the EVAP canister purge line at the underbody and look for liquid fuel in the line.

| Important: If the liquid fuel is present in the canister, it must be replaced.

• | If the liquid fuel is present, install a siphon hose on this line and attempt to draw out more fuel.

• | If fuel is in the canister, investigate the vapor venting of the system. Refer to Diagnosing Fuel Filling Problems.

2. The EVAP purge solenoid function - Check for DTCs and refer to the appropriate code in Engine/Emissions Controls section of this service manual.

Evidence of fuel loss or fuel vapor odor can be caused by:

• | A cracked or damaged EVAP canister

• | A fuel saturated EVAP canister