For 1990-2009 cars

## Rear Compartment Lid Lock Cylinder Replacement Sedan

### Removal Procedure

1. Remove the rear applique. Refer to Rear Compartment Lid Applique.
2. Disconnect the latch cable from the lock cylinder assembly.
3. Remove the retainer clip from the lock cylinder assembly.
4. Remove the cylinder assembly.

### Installation Procedure

1. Position the cylinder assembly in the rear decklid.
2. Install the retainer clip.
3. Reconnect the latch cable to the lock cylinder assembly.
4. Install the rear applique. Refer to Rear Compartment Applique.