For 1990-2009 cars

Figure 1: |

#### Oil Pump Base Fluid Passages - Control Valve Body Side

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 2: |

#### Control Valve Body Fluid Passages (Oil Pump Base Side)

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(6) | Release
(13) | PRND4
(25) | Reverse
(28) | Drive
(41) | D21
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 3: |

#### Control Valve Body Fluid Passages (Channel Plate Side)

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12) | Lo/PRN
(12) | Lo/PRN
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(16) | 1-2 Signal
(16) | 1-2 Signal
(16) | 1-2 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(19) | VBS Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(31) | Filtered 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(40) | Coast Clutch
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 4: |

#### Control Valve Body to Spacer Plate Gasket

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(11) | PRN
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(16) | 1-2 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(19) | VBS Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(31) | Filtered 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 5: |

#### Spacer Plate

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12/11) | Lo/PRN/PRN
(12) | Lo/PRN
(12/44) | Lo/PRN/Lo
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15/16) | Filtered Actuator Feed/1-2 Signal
(17/15) | 2-3 Signal/Filtered Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20/21) | 1-2/3-4 Accumulator/1-2 Accumulator Feed
(20/21) | 1-2/3-4 Accumulator/1-2 Accumulator Feed
(20/22) | 1-2/3-4 Accumulator/3-4 Accumulator Feed
(20/22) | 1-2/3-4 Accumulator/3-4 Accumulator Feed
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(23/24) | 2-3 Accumulator/2-3 Accumulator Feed
(23/24) | 2-3 Accumulator/2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25/26) | Reverse/Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(29/28) | Forward Clutch/Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30/31) | 2-3 Drive/Filtered 2-3 Drive
(30/32) | 2-3 Drive/2nd Clutch
(30/32) | 2-3 Drive/2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35/36) | 3-4 Drive/Direct Clutch Feed
(35/36) | 3-4 Drive/Direct Clutch Feed
(36) | Direct Clutch Feed
(37/36) | Direct Clutch/Direct Clutch Feed
(37/36) | Direct Clutch/Direct Clutch Feed
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45/46) | Exhaust/Orificed Exhaust
(45/46) | Exhaust/Orificed Exhaust
(47) | Void

Figure 6: |

#### Spacer Plate to Channel Plate Gasket

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12) | Lo/PRN
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(29) | Forward Clutch
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void

Figure 7: |

#### Channel Plate Fluid Passages (Control Valve Body Side)

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(7) | Apply
(7) | Apply
(7) | Apply
(8) | Cooler
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(11) | PRN
(11) | PRN
(11) | PRN
(11/45) | PRN/Exhaust
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(37) | Direct Clutch
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(40) | Coast Clutch
(41) | D21
(41) | D21
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(#1) | Ball Check Valve
(#2) | Ball Check Valve
(#3) | Ball Check Valve
(#4) | Ball Check Valve
(#5) | Ball Check Valve
(#6) | Ball Check Valve
(#7) | Ball Check Valve

Figure 8: |

#### Channel Plate Fluid Passages (Case Side)

(1) | Suction
(1) | Suction
(2) | Line
(3) | Decrease
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(28) | Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(40) | Coast Clutch
(43) | Intermediate Band
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void

Figure 9: |

#### Channel Plate to Case Gasket

(1) | Suction
(1) | Suction
(2) | Line
(8) | Cooler
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(32) | 2nd Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(43) | Intermediate Band
(43) | Intermediate Band
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void

Figure 10: |

#### Case and Driven Sprocket Support Fluid Passages (Channel Plate Side)

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(8) | Cooler
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(37) | Direct Clutch
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(40) | Coast Clutch
(40) | Coast Clutch
(43) | Intermediate Band
(43) | Intermediate Band
(45) | Exhaust
(47) | Void
(47) | Void
(48) | Oil Level Control
(48) | Oil Level Control

Figure 11: |

#### Case Fluid Passages - Bottom

(1) | Suction
(10) | Lube 2
(10) | Lube 2
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(29) | Forward Clutch
(29) | Forward Clutch
(38) | 4th Band
(43) | Intermediate Band
(47) | Void
(47) | Void
(47) | Void
(48) | Oil Level Control
(48) | Oil Level Control

Figure 1: |

#### Oil Pump Base Fluid Passages - Control Valve Body Side

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 2: |

#### Control Valve Body Fluid Passages - Oil Pump Base Side

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(6) | Release
(13) | PRND4
(25) | Reverse
(28) | Drive
(41) | D21
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 3: |

#### Control Valve Body Fluid Passages (Channel Plate Side)

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12) | Lo/PRN
(12) | Lo/PRN
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(16) | 1-2 Signal
(16) | 1-2 Signal
(16) | 1-2 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(19) | VBS Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(31) | Filtered 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(40) | Coast Clutch
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 4: |

#### Control Valve Body to Spacer Plate Gasket

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(11) | PRN
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(16) | 1-2 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(31) | Filtered 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 5: |

#### Spacer Plate - Without Electronic Range Select Mode

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12/11) | Lo/PRN/PRN
(12) | Lo/PRN
(12/44) | Lo/PRN/Lo
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15/16) | Filtered Actuator Feed/1-2 Signal
(17/15) | 2-3 Signal/Filtered Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20/21) | 1-2/3-4 Accumulator/1-2 Accumulator Feed
(20/21) | 1-2/3-4 Accumulator/1-2 Accumulator Feed
(20/22) | 1-2/3-4 Accumulator/3-4 Accumulator Feed
(20/22) | 1-2/3-4 Accumulator/3-4 Accumulator Feed
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23/24) | 2-3 Accumulator/2-3 Accumulator Feed
(23/24) | 2-3 Accumulator/2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25/26) | Reverse/Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(29/28) | Forward Clutch/Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30/32) | 2-3 Drive/2nd Clutch
(30/32) | 2-3 Drive/2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35/36) | 3-4 Drive/Direct Clutch Feed
(35/36) | 3-4 Drive/Direct Clutch Feed
(36) | Direct Clutch Feed
(37/36) | Direct Clutch/Direct Clutch Feed
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45/46) | Exhaust/Orificed Exhaust
(45/46) | Exhaust/Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 6: |

#### Spacer Plate with Bonded Gaskets - With Electronic Range Select Mode

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(16) | 1-2 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(29) | Forward Clutch
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void

Figure 7: |

#### Spacer Plate to Channel Plate Gasket

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(8) | Cooler
(10) | Lube 2
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(12) | Lo/PRN
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(15) | Filtered Actuator Feed
(15) | Filtered Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(29) | Forward Clutch
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(35) | 3-4 Drive
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(41) | D21
(41) | D21
(42) | Intermediate Band Feed
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void

Figure 8: |

#### Channel Plate Fluid Passages (Control Valve Body Side)

(1) | Suction
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(2) | Line
(3) | Decrease
(4) | Converter Feed
(4) | Converter Feed
(5) | TCC Feed Limit
(5) | TCC Feed Limit
(6) | Release
(6) | Release
(6) | Release
(7) | Apply
(7) | Apply
(7) | Apply
(7) | Apply
(8) | Cooler
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(11) | PRN
(11) | PRN
(11) | PRN
(11) | PRN
(11/45) | PRN/Exhaust
(12) | Lo/PRN
(13) | PRND4
(13) | PRND4
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(14) | Actuator Feed
(17) | 2-3 Signal
(17) | 2-3 Signal
(18) | Torque Signal
(18) | Torque Signal
(18) | Torque Signal
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(20) | 1-2/3-4 Accumulator
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(23) | 2-3 Accumulator
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(30) | 2-3 Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(32) | 2nd Clutch
(33) | TCC Signal (PWM)
(34) | TCC Regulated Apply
(35) | 3-4 Drive
(36) | Direct Clutch Feed
(36) | Direct Clutch Feed
(37) | Direct Clutch
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(39) | D321
(39) | D321
(39) | D321
(40) | Coast Clutch
(40) | Coast Clutch
(41) | D21
(41) | D21
(42) | Intermediate Band Feed
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(43) | Intermediate Band
(44) | Lo
(44) | Lo
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(46) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(#1) | Ball Check Valve
(#2) | Ball Check Valve
(#3) | Ball Check Valve
(#4) | Ball Check Valve
(#5) | Ball Check Valve
(#6) | Ball Check Valve
(#7) | Ball Check Valve

Figure 9: |

#### Channel Plate Fluid Passages - Case Side

(1) | Suction
(1) | Suction
(2) | Line
(3) | Decrease
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(21) | 1-2 Accumulator Feed
(22) | 3-4 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(28) | Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(36) | Direct Clutch Feed
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(40) | Coast Clutch
(43) | Intermediate Band
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void

Figure 10: |

#### Channel Plate to Case Gasket

(1) | Suction
(1) | Suction
(2) | Line
(8) | Cooler
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(32) | 2nd Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(43) | Intermediate Band
(43) | Intermediate Band
(45) | Exhaust
(47) | Void
(47) | Void
(47) | Void

Figure 11: |

#### Case and Driven Sprocket Support Fluid Passages - Channel Plate Side

(1) | Suction
(1) | Suction
(1) | Suction
(2) | Line
(8) | Cooler
(8) | Cooler
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(9) | Lube 1
(10) | Lube 2
(10) | Lube 2
(24) | 2-3 Accumulator Feed
(24) | 2-3 Accumulator Feed
(25) | Reverse
(25) | Reverse
(26) | Reverse Clutch
(26) | Reverse Clutch
(27) | Lo Band
(27) | Lo Band
(28) | Drive
(28) | Drive
(32) | 2nd Clutch
(32) | 2nd Clutch
(37) | Direct Clutch
(37) | Direct Clutch
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(38) | 4th Band
(40) | Coast Clutch
(40) | Coast Clutch
(43) | Intermediate Band
(43) | Intermediate Band
(45) | Exhaust
(47) | Void
(47) | Void
(48) | Oil Level Control
(48) | Oil Level Control

Figure 12: |

#### Case Fluid Passages - Bottom

(1) | Suction
(10) | Lube 2
(10) | Lube 2
(25) | Reverse
(25) | Reverse
(27) | Lo Band
(27) | Lo Band
(29) | Forward Clutch
(29) | Forward Clutch
(38) | 4th Band
(43) | Intermediate Band
(47) | Void
(47) | Void
(47) | Void
(48) | Oil Level Control
(48) | Oil Level Control