For 1990-2009 cars

### Removal Procedure

#### Left Side Shown, Right Side Similar

1. Place the height adjuster to the lowest position.
2. Remove the center pillar weatherstrip/cover to expose the adjuster attaching fasteners.
3. Remove the shoulder belt height adjuster fasteners.
4. Remove the upper center pillar fastener. Partially remove the upper and lower trim moldings from the center pillar.
5. Pull on height adjuster to disengage attaching clip.
6. Pull on height adjuster to release the pin and remove from the height adjuster.
7. Temporarily install height adjuster onto center pillar. Hand tighten the fasteners.
8. Remove the shoulder belt fastener from the height adjuster.
9. Remove the fasteners and remove the height adjuster.

### Installation Procedure

1. Temporarily install shoulder belt height adjuster to the center pillar. Hand tighten, but do not torque the fasteners.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the top of the shoulder belt assembly to the height adjuster with the shoulder belt bolt.

Tighten
Tighten the bolt to 29 N·m (21 lb ft).

3. Install the height adjuster fasteners and install the height adjuster to the center pillar.
4. Align the lower hole to the hinged retainer clip and snap the adjuster into the clip.
5. Align the upper retaining pins into the slider assembly and snap the adjuster into place.
6. If the shoulder belt has come off the belt guide, install the shoulder belt behind the shoulder belt guide.
7. Install the upper B-pillar molding and fastener, then install the plug.

Tighten
Tighten the fastener to 10 N·m (89 lb in).

8. Install the height adjuster fasteners.

Tighten
Tighten the fasteners to 35 N·m (26 lb ft).

9. Install the outside weatherstrip to the center pillar.
10. Position the door weatherstrip over the center pillar molding
11. Test the height adjuster for the proper operation.