For 1990-2009 cars

#### Fluid Capacity Specifications (4T40-E)

Application | Specification
--- | ---
Metric | English
Bottom Pan Removal | 6.5 liters | 6.9 quarts
Complete Overhaul | 9.0 liters | 9.5 quarts
Dry | 12.2 liters | 12.9 quarts
Measurements are approximate.

Service Procedure | Capacities
--- | ---
Metric | English
Bottom Pan Removal | 6.5 L | 6.9 qt
Complete Overhaul | 9.0 L | 9.5 qt
Dry | 12.2 L | 12.9 qt
Measurements are approximate