For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Strut-to-Knuckle

- Initial Torque

50 N·m

37 lb ft

- Final Torque

100 N·m

74 lb ft

Inner Tie Rod-to-Outer Tie Rod Jam Nuts | 60 N·m | 44 lb ft
Rear Axle Control Arm Bracket-to-Body Bolts | 90 N·m + 30-45 degrees | 66 lb ft + 30-45 degrees
Wheel Bolts

- Initial Torque

63 N·m

46 lb ft

- Final Torque

125 N·m

92 lb ft