For 1990-2009 cars

### Removal Procedure

1. Remove the front door outer panel. Refer to Front Door Outer Panel removal procedure .

Important: Apply only enough tension so that the sound insulator panel releases from the door structure.

2. Remove the front insulator.

### Installation Procedure

Important: Make sure the attaching points are clean and dry. If the insulator panel has been damaged during removal, it must be replaced.

1. Install the front insulator using the locating holes and position the insulator panel to the structure. Make sure proper alignment is achieved. Improper alignment could cause outer panel misalignment.
2. Install the front door outer panel. Refer to Front Door Outside Panel installation procedure .