For 1990-2009 cars

### Removal Procedure

Caution: Refer to Glass and Sheet Metal Handling Caution in the Preface section.

1. Place your fingers as far as possible behind the mirror face toward the center of the back.
2. Remove the mirror face from the mirror housing with sufficient force to disengage the snap-locks on the mirror motor.
3. Remove the mirror face from the mirror housing.

### Installation Procedure

1. Position the mirror face to the mirror motor.
2. Install the mirror face to the mirror motor with the palm of the hand on the center of the glass, pressing in until fully seated.
3. Inspect the mirror for proper operation.