For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Disconnect the manifold absolute pressure (MAP) sensor harness connector.
3. Remove the MAP sensor attachment bolt and remove the MAP sensor with the grommet.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Make sure the MAP sensor mounting surface is clean. Install the MAP sensor with the grommet and attachment bolt.

Tighten
Tighten the manifold absolute pressure sensor bolt to 5 N·m (44 lb in).

2. Connect the MAP sensor harness connector. Push the connector in until the lock position is felt, then pull back to confirm engagement.