For 1990-2009 cars

### Removal Procedure

1. Remove the mirror trim cover by pulling out at the top.
2. Remove the foam filler.
3. Remove the nuts from the mirror.
4. Remove the mirror from the door.

### Installation Procedure

1. Position the mirror to the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the mirror.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the foam filler.
4. Install the mirror trim panel by placing the lower portion of the cover behind the trim panel and push in on the top fastener.