For 1990-2009 cars

### Removal Procedure

Important: Windshield lower molding locator can only be replaced by removing the windshield and then removing and installing a new windshield moldings, upper, lower locator and both "A" pillar moldings.

1. Remove windshield. Refer to "Windshield" removal in this section.
2. Remove lower locator windshield molding from windshield.
3. Clean old adhesive from glass using isopropyl alcohol.

### Installation Procedure

1. Install windshield lower locator and upper reveal molding.

Important: Adhesive is already in service part. No additional adhesive is necessary.

2. Install windshield. Refer to "Windshield" installation in this section.