For 1990-2009 cars

### Removal Procedure

1. Using a grease pencil, mark around the striker for installation purposes.
2. Remove the screws.
3. Remove the striker and striker shim if present.

### Installation Procedure

1. Install the striker and striker shim, if present, loosely with bolts.
2. Align the striker with the marks made prior to removal.
3. Hand tighten the bolts.
4. Inspect the door closing. Align the striker as required.

Notice: Refer to Fastener Notice in the Preface section.

5. Tighten the striker bolts.

Tighten
Tighten the door striker bolts to 20 N·m (15 lb ft).