For 1990-2009 cars

## Tail Lamp Replacement Wagon

### Removal Procedure

1. Open the liftgate.
2. Remove interior rear access panel.
3. Remove the nuts from the tail lamp.
4. Disconnect the electrical connector from the tail lamp.
5. Remove the tail lamp by pulling straight back.

### Installation Procedure

1. Connect the electrical connector to the tail lamp.
2. Position the tail lamp to the quarter panel pressing in until fully seated.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts to the tail lamp.

Tighten
Tighten the nuts to 3.5 N·m (31 lb in).

4. Install interior access panel.
5. Close the liftgate.

## Tail Lamp Replacement Sedan

### Removal Procedure

1. Open the rear compartment.
2. Pull back the side carpet to gain access to the tail lamp.
3. Remove the nuts from the tail lamp.
4. Gently pull the tail lamp housing straight back.
5. Disconnect the electrical connector from the tail lamp.

### Installation Procedure

1. Connect the electrical connector to the tail lamp.
2. Position tail lamp to the quarter panel and push in until fully seated.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts to the tail lamp.

Tighten
Tighten the nuts to 3.5 N·m (31 lb in).

4. Reposition the side carpet.
5. Close the rear compartment.