For 1990-2009 cars

#### Tools Required

• | KM-907 Control Arm Bushing Remover/Installer

• | KM-508-A Control Arm Bushing Remover/Installer

• | KM-671 Bushing Remover/Installer

### Disassembly Procedure

1. Using special tools KM-508A-3 and KM-508-1, press out the front bushing.
2. Using special tools KM-907-21, KM-907-22, and KM-671 , press out the rear control arm bushing.

### Assembly Procedure

1. Using bushing press KM-508-1, KM-508-2, and KM-508-3, press in the front control arm bushing.
2. Using special tools KM-907-23, KM-907-24, and KM-671 , press in the rear control arm bushings.