For 1990-2009 cars

### Removal Procedure

1. Remove the 3 lower steering column trim cover from the steering column attachment screws.
2. Remove the upper steering column trim cover.
3. Remove the ignition switch bezel.
4. Remove the lock cylinder bezel from the steering column shroud by carefully prying with a thin-bladed screwdriver.
5. Remove the lower steering column trim cover.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the steering column trim cover and attachment fasteners.

Tighten
Tighten the steering column trim cover attaching fasteners to 4 N·m (35 lb in).

2. Install the ignition switch bezel.