For 1990-2009 cars

## Rear Door Frame Applique Replacement Sedan /Wagon

### Removal Procedure

1. Remove the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
2. Slide the applique up.
3. Remove the applique by tilt the front edge out evenly and pull out from the door window frame.

### Installation Procedure

1. Position the applique to the slots in the rear door window frame.
2. Slide the applique into the slots , moving slightly forward and down.
3. Install the rear door outer belt seal. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .

## Rear Door Frame Applique Replacement Rear

### Removal Procedure

1. Remove the outer belt seal. Refer to Outer Belt Seal - Front Removal.
2. Slide applique up.
3. Tilt the front edge out evenly and pull out to remove.

### Installation Procedure

1. Slide the applique into the slots and move slightly forward and down.
2. Install the outer belt seal. Refer to Outer Belt Seal Installation.