For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion and the rear seat back assemblies. Refer to Rear Seat Cushion Cover and Pad Replacement .
2. Remove the rear seat back outer pivot bolt.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat back outer pivot bolt.

Tighten
Tighten the rear seat back outer pivot bolt to 20 N·m (15 lb ft).

2. Install the rear seat cushion and the rear seat back assemblies. Refer to Rear Seat Cushion Cover and Pad Replacement .