For 1990-2009 cars

### Removal Procedure

1. Disconnect the fuel pressure regulator hose from the throttle body and fuel rail.
2. Remove the throttle body.
3. Remove the fuel pipes and clip.
4. Remove the fuel rail assembly.
5. Remove the knock sensor connector from the intake manifold.
6. Remove the knock sensor.
7. Remove the intake manifold retaining nuts and bolts.
8. Remove the intake manifold.
9. Remove the intake manifold gasket. The gasket is reusable if it is not damaged.
10. If the intake manifold needs to be replaced, transfer the following parts:

• | The throttle body

• | The body gasket. The manifold to throttle body gasket is reusable if it is not damaged.