For 1990-2009 cars

# Proper Tool for Removal and Installation of Oil Filter Cap

Subject: | Service Information Regarding Proper Tool for Removal and Installation of Oil Filter Cap.

Models: | 2000 - 2001 Saturn L-Series vehicles equipped with 2.2 L 4 cylinder (L61) engine

### Purpose

The purpose of this bulletin is to provide service information regarding proper tools for removal and installation of oil filter cap on all 2000 - 2001 Saturn L-Series vehicles equipped with 2.2L 4 cylinder (L61) engines. Proper tool must be used for removal and installation in order to prevent damage to oil filter cap resulting in an oil leak.

### Service Procedure

The oil filter cap has two features that can be used for removal and installation purposes:

• | 32 mm hex molded into top of the oil filter cap.

• | 14 flat feature incorporated into the outer rim of the cap, the diameter of the flats is 68 mm.

| Notice: If adjustable or open end wrench is used on the 32 mm hex feature, damage to oil filter cap can result causing oil leak. There are two acceptable tools that may be used for removal and installation of oil filter cap.

• | 32 mm socket for hex feature

• | Cap style oil filter wrench for 14 flat feature on rim of oil filter cap.

### Parts Requirements

The following is a list of cap style oil filter wrenches (or equivalent) that will work on 14 flat feature on oil filter cap.

Manufacturer | Part Number
--- | ---
Matco | OFW6814
Ritefit | G-A256
Mac | OF6814

Important: Saturn Cooperation believes the above list of tools to be reliable. there may be additional manufactures of such tools. Saturn Corporation does not endorse, indicate any preference for, or assume responsibility for the above list of tools from these firms or for any such tools which may be available from other sources.