For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Carefully peel off.
3. Remove the front door outer panel.
4. Disconnect the electrical connectors from the power door lock, power mirror, power window, and speaker, if equipped.
5. Remove the wiring retainers from the door structure.
6. Remove 2 rubber grommets.
7. Remove the wiring harness.

### Installation Procedure

1. Install the wiring harness.
2. Install 2 rubber grommets.
3. Install the wiring retainers to the door structure.
4. Connect the electrical connectors to the power door lock, power mirror, power window, and speaker, if equipped.
5. Install the front door outer panel.

Important: Replace the water deflector if damaged.

6. Install the water deflector.
7. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .