For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Pull back the rear door water deflector away from the handle area. Refer to Rear Side Door Water Deflector Replacement .
3. Slide the door handle forward and then outward.
4. Twist the door handle to unhook the door handle rod.

### Installation Procedure

1. Twist the door handle to hook the door handle rod into the handle.
2. Install the door handle into the slots and slide forward.
3. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .