For 1990-2009 cars

### Removal Procedure

1. Squeeze park brake boot in locations shown in illustration to disengage park brake boot.
2. Lift up on park brake boot, pull over park brake lever assembly and remove park brake boot.

### Installation Procedure

1. Pull park brake boot over park brake lever.
2. Position park brake boot over console and push at snap locations to engage park brake boot to console.