For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Outlet to I/P Fastener | 2.5 N·m | 22 lb in
Ashtray to Center Console Fasteners | 2 N·m | 18 lb ft
Console Arm Rest Fasteners | 2.5 N·m | 22 lb in
Console Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Bin to I/P Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Door Fasteners | 2 N·m | 18 lb in
Glove Compartment Door Outer Cover Fasteners | 2 N·m | 18 lb in
Glove Compartment Latch Fasteners | 2 N·m | 18 lb in
HVAC Control Head to I/P Fasteners | 2.5 N·m | 22 lb in
I/P Assembly to Vehicle Attaching Fasteners | 20 N·m | 15 lb ft
I/P Cluster Trim Plate to I/P Housing Fasteners | 2.5 N·m | 22 lb in
I/P to Floor Pan Bracket Nuts | 20 N·m | 15 lb ft
Radio Ground Strap to H-Brace Stud Fasteners | 6 N·m | 53 lb in
Radio to I/P Fasteners | 2.5 N·m | 22 lb in
Steering Column Trim Cover Attaching Fasteners | 4 N·m | 35 lb in
Steering Wheel Attaching Nut | 40 N·m | 30 lb ft