For 1990-2009 cars

#### Tools Required

J 41742 Connecting Rod Guide

### Removal Procedure

1. Rotate the crankshaft to a position where the connecting rod bolts are most accessible.
2. Mark the connecting rod and cap with the cylinder position. Also mark their orientation. This will ensure that caps and connecting rods are re-assembled properly.
3. Remove any ridge at the top of the cylinder bore to avoid damage to the piston ring lands.
4. Remove the connecting rod bolts.
5. Remove the connecting rod cap.
6. Install the J 41742 in the connecting rod bolt holes before removing the piston and connecting rod assembly.
7. Remove the piston and connecting rod assembly.
8. Complete steps 2-7 for the remaining pistons and connecting rods.