For 1990-2009 cars

### Circuit Description

The vehicle option content information must be entered as a part of the body control module (BCM) programming procedure. If the vehicle option content information is not included and the programming procedure is complete, the DTC will set.

### Conditions for Setting the DTC

• | Programming of the BCM was completed without completing the vehicle option content information

• | Last 4 digits of the SDM part number

• | If the SDM was replaced without programming the BCM

### Diagnostic Aids

• | Refer to the Saturn Service Stall System (SSS) users guide for programming the BCM. Include the proper options for the vehicle.

• | Check for the proper SDM part number.