For 1990-2009 cars

### Removal Procedure

#### Left Side Shown, Right Side Similar

1. Remove the rear seat bolster.

• | Reach down into the corner of the rear seat cushion to expose the bolster retaining tab.

• | Bend the bolster retaining tab upward.

• | Lower the rear seat back.

• | Starting at the bottom, pull forward to disengage the bolster from the retaining tab then pull upward to disengage the upper attachment.

2. Remove the shoulder belt from the comfort guide.
3. Remove the comfort guide retainer and remove the comfort guide.

### Installation Procedure

1. Install the comfort guide with the comfort guide retainer.
2. Install the comfort guide to the shoulder belt.

Caution: Make sure the rear seat shoulder belt is not caught behind the bolster when installing the bolster.

3. Install the rear seat bolster.

• | Position the bolster onto the upper bolster attachment.

• | Push down on the bolster to engage the upper attachment and push the bolster back over the retaining tab.

• | Bend the retaining tab down to fasten the bolster.

• | Raise the rear seat back.

4. Check the function of the rear seat shoulder belt assembly for the proper operation.