For 1990-2009 cars

### Removal Procedure

1. Flip the load floor side-wings upwards.
2. Lift the load floor upwards.
3. Slide the load floor tabs out of the front load floor assembly.
4. Lift the load floor out of the vehicle.

### Installation Procedure

1. Position the load floor into the vehicle.
2. Slide the load floor tabs into the front load floor assembly.
3. Lower the load floor.
4. Reposition the load floor side wings.