For 1990-2009 cars

### Removal Procedure

1. Remove the driver side rear seat back assembly. Refer to Rear Split Folding Seat Back Replacement .
2. Remove the rear seat back beam. Refer to Seat Back Latch Beam Replacement - Rear .
3. Remove the rear seat back cover/pad.
4. Drill out the rivets and remove the rear seat back latch assembly.

### Installation Procedure

1. Install the rear seat back latch assembly with the rivets.
2. Install the rear seat back cover/pad.
3. Install the rear seat back beam. Refer to Seat Back Latch Beam Replacement - Rear .
4. Install the rear seat back assembly. Refer to Rear Split Folding Seat Back Replacement .