For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Control Assembl-to-Brackets Nuts | 20 N·m | 15 lb ft
ABS Control Unit Connection | 16 N·m | 12 lb ft
Accelerator Pedal Bracket Nuts | 10 N·m | 89 lb in
Adjuster Jam Nut-to-Brake Booster Push Rod Connector | 18 N·m | 13 lb ft
Brake Booster Bracket Attachment Nuts | 18 N·m | 13 lb ft
Brake Booster-to-Brake Booster Bracket Bolts | 20 N·m | 15 lb ft
Brake Caliper-to-Steering Knuckle Bolts | 95 N·m | 70 lb ft
Brake Drum Retaining Fastener | 4 N·m | 35 lb in
Brake Hose Connection | 16 N·m | 12 lb ft
Brake Hose-to-Brake Pipe | 16 N·m | 12 lb in
Brake Hose-to-Caliper (use new washer) | 40 N·m | 30 lb ft
Brake Pedal Bracket-to-I/P Support Beam Nuts | 20 N·m | 15 lb ft
Brake Pipe Bracket-to-Rear Axle Control Arm | 8 N·m | 71 lb in
Brake Pipe Bracket-to-Rear Control Arm | 8 N·m | 71 lb in
Brake Pipe Fitting Connection | 16 N·m | 12 lb ft
Brake Pipe-to-Master Cylinder Nuts | 16 N·m | 12 lb ft
Brake Pipe-to-Proportioning Valve | 16 N·m | 12 lb ft
Brake Pipe-to-Rear Caliper | 16 N·m | 12 lb ft
Brake Pipe-to-Rear Wheel Cylinder | 16 N·m | 12 lb ft
Brake Pipes-to-Manifold Valve | 16 N·m | 12 lb ft
Brake Pipes-to-Master Cylinder | 18 N·m | 13 lb ft
Brake Rotor Retaining Fastener | 4 N·m | 35 lb in
Brake Rotor Retaining Screw | 4 N·m | 35 lb in
Caliper Bleeder Valve | 6 N·m | 53 lb in
Caliper-to-Bracket Guide Pins | 30 N·m | 22 lb ft
Console Fasteners (Front and Rear) | 2.5 N·m | 22 lb in
Exhaust Heat Shield-to-Body Fasteners | 4 N·m | 35 lb in
Female Connector | 16 N·m | 12 lb ft
Female Repair Union-to-Vehicle Fitting | 16 N·m | 12 lb ft
Front Brake Pipe Connection (ABS) | 16 N·m | 12 lb ft
Front Caliper Bleeder Valves | 8 N·m | 71 lb ft
Intermediate Steering Shaft Pinch Bolt | 30 N·m | 22 lb ft
Manifold Valve Connection (Non-ABS) | 16 N·m | 12 lb ft
Manifold Valve-to-Vehicle Bolt | 5 N·m | 44 lb in
Master Cylinder-to-Brake Booster Nuts | 25 N·m | 18 lb ft
Park Brake Alarm Fastener | 2.5 N·m | 22 lb in
Park Brake Lever-to-Floor Pan Nuts | 10 N·m | 89 lb in
Proportioning Valve Connection | 16 N·m | 12 lb ft
Rear Brake Hose Connection | 16 N·m | 12 lb ft
Rear Caliper Bleeder Valve | 6 N·m | 53 lb in
Rear Caliper-to-Rear Axle Control Arm Bolts | 80 N·m | 59 lb ft
Rear Caliper-to-Rear Axle Control Arm | 80 N·m | 59 lb ft
Rear Crossover Connection | 16 N·m | 12 lb ft
Rear Hub Assembly-to-Knuckle Nuts | 50 N·m +30° to 45° | 37 lb ft +30° to 45°
Rear Wheel Cylinder Bleeder Valve | 8 N·m | 71 lb in
Resonator Pipe-to-Exhaust Manifold Pipe | 20 N·m | 15 lb ft
Wheel Bolts (Final Torque) | 125 N·m | 92 lb ft
Wheel Bolts (Initial Torque) | 63 N·m | 46 lb ft
Wheel Cylinder-to-Backing Plate Bolt | 9 N·m | 80 lb in
Wheel Speed Sensor Bracket-to-Steering Knuckle | 8 N·m | 71 lb in
Wheel Speed Sensor-to-Steering Sensor Bracket | 8 N·m | 71 lb in