For 1990-2009 cars

## Luggage Carrier Replacement Wagon

### Removal Procedure

Important: Remove and replace one side of the luggage carrier at a time. The headliner should be completely reinstalled before removing the opposite side luggage carrier to ensure proper alignment of the headliner.

1. Starting with the upper clip locators, remove the windshield pillar trim by gently pulling on the trim.
2. Remove the screws from the sunshade and remove the sunshade.
3. If the vehicle is equipped with an illuminated sunshade, disconnect the electrical connection.
4. Remove the sunshade inner retainer clips.
5. Remove the assist handle by pulling down on the handle to expose the fasteners and remove the fasteners.
6. On vehicles with an illuminated assist handle, disconnect the wiring harness connection.
7. Remove the coat hook cover to expose the coat hook fastener.
8. Remove the coat hook.
9. Loosen the molding at the top rear area of the vehicle by pulling on the left and right side quarter glass upper moldings.
10. Disengage the attaching clips by pulling on the headliner rear molding and remove the molding.
11. Remove the cargo shade.
12. Lower the rear seat back assembly.
13. Remove the molding by pulling gently at the attaching clip locations.
14. Remove the rear seat upper shoulder belt fastener cover.
15. Remove the rear seat upper shoulder belt fastener to remove the shoulder belt.
16. Starting at the front edge of the molding, pull at the attaching clips to remove the molding assembly.
17. Remove the center pillar upper trim moldings.
18. Disengage the dome lamp hook-and-loop fastener from the roof structure by reaching in the door opening above the headliner to the center dome lamp.
19. Gently pull down on the headliner to provide clearance for nut access.
20. Remove the nuts attaching the luggage carrier to the roof.
21. Remove the luggage carrier from the roof.

### Installation Procedure

1. Install the pads and the seals over the luggage carrier studs at all mounting locations.
2. Position the luggage carrier studs through the holes in the roof.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts holding the luggage carrier to the roof and tighten.

Tighten
Tighten the luggage carrier-to-roof panel nuts to 20 N·m (15 lb ft).

4. Install the sunshade inner retainer clip.

Tighten
Tighten the sunshade inner retainer clip fastener to 15 N·m (11 lb ft).

5. On vehicles equipped with an illuminated sunshade, connect the sunshade wiring harness.
6. Install the sunshade assembly.

Tighten
Tighten the sunshade fasteners to 15 N·m (11 lb ft).

7. On vehicles equipped with illuminated assist handles, connect the assist handle lamp wiring harness.
8. Install the assist handle assembly.
9. Install the coat hooks.

Tighten
Tighten the coat hooks to 15 N·m (11 lb ft).

Caution: Apply Loctite 242® Threadlocker US P/N 12345382 (Canadian P/N 10953489), or equivalent, on all restraint bolts/nuts before installation. Failure to use such threadlocker correctly may result in personal injury.

10. Position the side molding at the attaching clips.
11. Secure the side molding by pushing gently at the clip locations.
12. Position the molding at the attaching clip locations.
13. Secure the molding by pushing gently at the clip locations.
14. Install the cargo shade.
15. Raise the rear seat back assembly.
16. Position the weather-strip over the cargo shade side cover.
17. Install the upper shoulder belt fastener.

Tighten
Tighten the upper shoulder belt fastener to 35 N·m (26 lb ft).

18. Snap the upper shoulder belt fastener cover into place.
19. Raise the rear seat back assembly.
20. Apply the weather-strip over the front and rear of the side molding using a flat blade tool.
21. Position the headliner rear molding at the attaching clip locations.
22. Snap the molding in place by gently pushing at the clip locations.
23. Install the left and right side quarter glass upper moldings.
24. Install the cargo shade.
25. Test the shoulder belt assembly to ensure proper operation.
26. Install the windshield pillar molding, the center pillar upper molding, and the C-pillar trim molding.
27. Install the weather-strip over the headliner assembly at all door locations using a small flat blade tool.