For 1990-2009 cars

### Removal Procedure

1. On vehicles equipped with L81 engines, remove the rear exhaust manifold pipe heat shield.
2. Remove the rear transaxle mount through bolt.
3. Remove one of three transaxle mount to frame bolts.

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

4. Raise the vehicle on a hoist.
5. Remove the remaining mount to frame attachment bolts.
6. Remove the rear mount from the vehicle.
7. Remove the transaxle mount bracket to the transaxle bolts.
8. Remove the transaxle mount bracket from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear transaxle mount bracket to the transaxle and tighten the fasteners.

Tighten
Tighten the rear transaxle mount bracket-to-transaxle bolts to 90 N·m (66 lb ft).

2. Install the transaxle mount to the frame attachment fasteners and tighten.

Tighten
Tighten the rear transaxle mount-to-frame to 60 N·m (44 lb ft).

3. Lower the vehicle from the hoist.
4. Install and tighten the transaxle mount to the frame attachment fastener.

Tighten
Tighten the rear transaxle mount-to-frame bolts to 60 N·m (44 lb ft).

Important: On L61 engines, be sure the transaxle mount heat shield is in place.

5. Install the transaxle mount to the engine mount bracket through bolt.

Tighten
Tighten the rear transaxle mount through bolt to 90 N·m (66 lb ft).

6. On vehicles equipped with L81 engines, install the rear exhaust manifold pipe heat shield.

Tighten
Tighten the exhaust manifold pipe heat shield bolts (L81) to 8 N·m (71 lb in).