For 1990-2009 cars

### Removal Procedure

1. Remove the steering column upper trim cover. Refer to Steering Column Trim Covers Replacement .
2. Remove the ignition switch fasteners.
3. Disconnect the electrical connectors.
4. Remove the ignition switch.

### Installation Procedure

1. Connect the electrical connectors.
2. Position the ignition switch.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the ignition switch fasteners.

Tighten
Tighten the ignition switch fasteners to 1.5 Nm (13 lb in).

4. Install the steering column upper trim cover. Refer to Steering Column Trim Covers Replacement .
5. Install the lock cylinder bezel.