For 1990-2009 cars

### Removal Procedure

1. Remove the center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages, and Console.
2. Remove the radio fasteners.
3. Pull the radio out slightly to access the rear of the radio.
4. Disconnect the electrical connectors, antenna, and radio ground strap spade terminal from the rear of the radio.
5. Remove the radio.

### Installation Procedure

1. Connect the radio ground strap spade terminal, electrical connectors, and antenna to the rear of the radio.
2. Install the radio by sliding it into the guides on the instrument panel (I/P).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the radio fasteners.

Tighten
Tighten the fasteners to 2.5 N·m (22 lb in).

4. Install the center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages, and Console.