For 1990-2009 cars

### Repair Procedure

1. Turn the ignition OFF.
2. Disconnect the MAP sensor harness connector.
3. Remove the throttle cable bracket attachment nuts. Pick the throttle cable bracket up and move it to the side to allow enough clearance to remove the MAP sensor.
4. Remove the MAP sensor and the MAP sensor port seal if it is still retained in the intake manifold

### Installation Procedure

1. Install the MAP sensor with the port seal into the intake manifold

Notice: Refer to Fastener Notice in the Preface section.

2. Install the throttle cable bracket and the attachment nuts.

Tighten
Tighten the throttle cable bracket nuts to 5 N·m (44 lb in).

3. Connect the MAP sensor harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.