For 1990-2009 cars

### Installation Procedure

The rearview mirror is attached to a support which is bonded to the windshield glass. This support is installed by the glass supplier using an autoclaving process.

Service replacement windshield glass has the mirror support bonded to the glass assembly. To install a detached mirror support the following items are needed:

• | P/N 11067-2, LOCTITE® Rearview Mirror Adhesive, or equivalent

• | Original mirror support

• | Wax marking pencil or crayon

• | Rubbing alcohol

• | Clean paper towel

• | Fine grade emery cloth or sandpaper (No. 320 or No. 360)

• | Clean toothpick

1. Center the support within the black-out area.
2. On the inside glass surface, clean the mirror support black-out area with paper towel and a domestic scouring cleanser, glass cleaning solution, or polishing compound. Rub until the area is completely clean and dry. When dry, clean the area with an alcohol saturated paper towel to remove any traces of scouring powder or cleaning solution from these area.
3. Separate the mirror from the support by loosening the screw and using a small blade screwdriver. With piece of fine grade emery cloth (No. 320 or No. 360) or sandpaper, sand the bonding surface of the rearview mirror support. All traces of factory installed adhesive must be removed prior to installation.
4. Wipe the sanded mirror support with clean paper towel saturated with alcohol and allow to dry.
5. Follow directions on the manufacturer's kit to prepare the rearview mirror support prior to installation on the glass.
6. Center the support within the black-out area with the rounded end pointed upward. Press the support against the glass for 30-60 seconds, exerting steady pressure against the glass. After 5 minutes, any excess adhesive may be removed with an alcohol moistened paper towel or glass cleaning solution.
7. Install the mirror and connect the electrical connection, if equipped.