For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Crossmember Nut and Bolt | 90 N·m + 60-75 degrees | 66 lb ft + 60-75 degrees
Exhaust Manifold Pipe-to-Exhaust Pipe Bolts | 20 N·m | 15 lb ft
Heat Shield-to-Rear Suspension Support | 8 N·m | 71 lb in
Park Brake Cable-to-Rear Knuckle | 8 N·m | 71 lb in
Rear Axle Control Arm Bracket-to-Body Bolts | 90 N·m + 30-45 degrees | 66 lb ft + 30-45 degrees
Rear Axle Control Arm Bracket-to-Knuckle | 90 N·m | 66 lb ft
Rear Brake Drum-to-Hub Screw | 4 N·m | 35 lb in
Rear Brake Line Bracket-to-Knuckle | 8 N·m | 71 lb in
Rear Caliper Mounting Bolts | 80 N·m | 59 lb ft
Rear Hub-to-Knuckle | 50 N·m + 30-45 degrees | 37 lb ft + 30-45 degrees
Rear Shock Absorber-to-Knuckle Bolt | 150 N·m + 30-45 degrees | 110 lb ft + 30-45 degrees
Rear Shock Carrier-to-Body Bolts | 55 N·m | 41 lb ft
Rear Stabilizer Bar Clamp-to-Cross Member | 55 N·m | 41 lb ft
Rear Stabilizer Bar-to-Knuckle | 55 N·m | 41 lb ft
Rear Suspension Control Arm-to-Knuckle | 90 N·m + 60-75 degrees | 66 lb ft + 60-75 degrees
Rear Suspension Control Arm-to-Rear Suspension Support | 90 N·m + 60-75 degrees | 66 lb ft + 60-75 degrees
Rear Suspension Support-to-Body Bolts | 90 N·m + 90-105 degrees | 66 lb ft + 90-105 degrees
Spring Seat Nut to Rear Shock Absorber Shaft | 20 N·m | 15 lb ft
Wheel Bolts

- Initial Torque

63 N·m

46 lb ft

- Final Torque

125 N·m

92 lb ft