For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion assembly. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the bracket attaching bolts and remove the brackets.

### Installation Procedure

1. Position the new brackets to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install new bracket attaching bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the rear seat cushion assembly. Refer to Rear Seat Cushion Replacement in Seats.