For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat back.
2. Remove the rear seat back latch bow fasteners and remove the bow.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat back latch bow fasteners and install the rear seat back latch bow.

Tighten
Tighten the rear folding seat back latch fasteners to 20 N·m (15 lb ft).

2. Raise the rear seat back assembly.