For 1990-2009 cars

### Removal Procedure

1. Raise the headrest assembly to the full up position.
2. Pull upward on the headrest while pushing the headrest button toward the rear of the vehicle and pull the headrest out of the seat back.

### Installation Procedure

1. Align the headrest support rods with the holes in the headrest sleeves.
2. Push the headrest into the sleeves to engage the support rods.