For 1990-2009 cars

# Front and Rear Suspension Torque Specifications

Subject: | Service Manual Update for 2000/2001 L-Series Chassis Service Manual Regarding Front and Rear Suspension Torque Specifications

Models: | 2000-2001 Saturn L-Series Vehicles

Attention: | Please distribute this bulletin to: All Technicians and Body Shop

### Purpose

The purpose of this bulletin is to update all 2000/2001 L-Series Chassis Service Manuals at your location.

Please obtain all the 2000/2001 L-Series Chassis Service Manuals at your location and make the necessary updates as indicated below.

• | On page 16 and 193, locate "Front Strut-to-Knuckle (final torque)" torque specification.

1. | Cross out 90 Nm and 66 ft-lbs.

2. | Write in 100 Nm and 73 ft-lbs.

• | On page 17 and 244, locate "Rear Axle Control Arm Bracket-to-Body Bolts" torque specfications and write in 30° - 45° after each torque specification.

• | On page 17 and 245, locate "Rear Hub-to-Knuckle" torque specfications and write in 30° - 45° after each torque specification.