For 1990-2009 cars

## Child Restraint Tether Anchor Replacement Sedan

### Removal Procedure

1. Remove the rear shelf panel.

Refer to the Rear Window Shelf Trim Panel Replacement .

2. Remove the child restraint bracket fastener and remove the bracket.

### Installation Procedure

Caution: Refer to Loctite Threadlocker on Restraint Fastener Caution in the Preface section.

1. Install the child restraint bracket with fastener.

Tighten
Tighten the child restraint bracket bolt to 20 N·m (15 lb ft).

2. Install the rear shelf panel.

Refer to Rear Window Shelf Trim Panel Replacement

## Child Restraint Tether Anchor Replacement Wagon

### Removal Procedure

1. Remove the load floor panel from the vehicle.
2. Remove the child restraint bracket fastener and remove the bracket.

### Installation Procedure

Caution: Refer to Loctite Threadlocker on Restraint Fastener Caution in the Preface section.

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child restraint fastener and the bracket to the vehicle.

Tighten
Tighten the child restraint bracket bolt to 20 N·m (15 lb ft).

2. Install the load floor panel.