For 1990-2009 cars

## DTC P0757 L61

### Circuit Description

The 1-2 shift solenoid valve (1-2 SS Valve) is a normally open exhaust valve that in conjunction with the 2-3 shift solenoid valve (2-3 SS Valve), allows four different shifting combinations. The 2-3 SS Valve is attached to the control valve body, within the transaxle. The PCM monitors the actual gear ratio and compares the actual gear ratio with the commanded gear ratio. The diagnostic will detect the following conditions: A stuck off 2-3 SS Valve, or a stuck off 2-3 Shift Valve. These conditions will cause the actual gear ratio to be different from the commanded; 2nd gear ratio in 3rd and 1st gear ratio in 4th and thus set DTC P0757.

### DTC Parameters

DTC P0757 will set if either of the following cases occur:

• | Commanded gear is 3rd, gear ratio is 1.54:-1.71:1, and engine torque is:

Engine Torque

• | MY 2002: 27-407 N·m (20-300 lb ft) for 3 seconds

• | MY 2003: 27-237 N·m (20-175 lb ft) for 3 seconds

• | Commanded gear is 4th, and gear ratio is 2.87:-3.13:1 and engine torque is:

Engine Torque

• | MY 2002: 27-407 N·m (20-300 lb ft) for 2 seconds

• | MY 2003: 27-237 N·m (20-175 lb ft) for 2 seconds

• | Engine is running

• | Ignition 1 is 8-18 volts

• | TP angle is greater than 8 percent

• | Transmission ISS is 150-6,000 RPM

• | Transmission OSS is greater than 150 RPM

• | Transmission range is not Park, Reverse, or Neutral

• | Transmission Fluid Temperature is 20-130°C (68-266°F)

• | No TP angle DTCs have set

• | The time since the last gear change is greater than 0.2 seconds

• | DTC P0502, P0503, P0716, P0717, P0753, P0758

• | MY 2002: DTC P1810 has not set

• | MY 2003: DTCs P0742 and P1860 have not set

DTC P0757 diagnostic runs continuously.

DTC P0757 is a type A DTC.

### Diagnostic Aids

• | The 2-3 shift solenoid valve is stuck off.

• | The 2-3 shift valve solenoid is leaking and is stuck off.

## DTC P0757 L81

### Circuit Description

The 1-2 shift solenoid vale (1-2 SS Valve) is a normally open exhaust valve that in conjunction with the 2-3 shift solenoid valve (2-3 SS Valve), allows four different shifting combinations. The 2-3 SS Valve is attached tot he control valve body, within the transaxle. The TCM monitors the actual gear ratio and compares the actual gear ratio with the commanded gear ratio. This diagnostic will detect the following conditions: A stuck off 2-3 SS Valve, or a stuck off 2-3 shift valve. These conditions will cause the actual gear ratio to be different from the commanded; 2nd gear ratio in 3rd and 1st gear ratio in 4th and thus set DTC P0757.

### DTC Parameters

DTC P0757 will set if either of the following cases occur:

• | Current gear is 3rd, gear ratio is 1.54:1-1.71:1, vehicle speed is greater than 8 km/h (5 mph), and engine torque is:

Engine Torque

• | MY 2002: 35-300 N·m (26-221 lb ft) for 3 seconds

• | MY 2003: 30-250 N·m (22-184 lb ft) for 3 seconds

• | Current gear is 4th, and gear ratio is 2.87:1-3.13:1, and vehicle speed is greater than 20 km/h (12 mph), and engine torque is:

Engine Torque

• | MY 2002: 0-300 N·m (0-221 lb ft) for 2 seconds

• | MY 2003: 0-250 N·m (0-184 lb ft) for 2 seconds when

• | TP angle is greater than 8 percent

• | MY 2002: Transmission range is not Park, Reverse, or Neutral

• | Transmission fluid temperature is 20-130°C (68-266°F)

• | Engine speed is:

- | MY 2002: 200-7,500 RPM for 5 seconds

- | MY 2003: 500-6,500 RPM for 5 seconds

• | MY 2002: Ignition 1 is 8-18 volts

• | No TP angle DTCs have set

• | DTC P0502, P0503, P0716, P0717, P1842, P1843, P1845, and P1847 have not set

• | MY 2002: DTC P1810 has not set

DTC P0757 diagnostic runs continuously.

DTC P0757 is a type A DTC.

### Diagnostic Aids

• | The 2-3 shift solenoid valve is stuck off.

• | The solenoid is leaking.

• | The 2-3 shift valve solenoid is leaking and is stuck off.