For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .
2. Remove the steering column trim cover. Refer to Steering Column Trim Covers Replacement in Steering Wheel and Column.
3. Move steering wheel to lowest position.
4. Remove the four fasteners.
5. Remove the cluster bezel.

### Installation Procedure

1. Install the cluster bezel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bezel fasteners.

Tighten
Tighten the bezel fasteners to 2.5 N·m (22 lb in).

3. Install the steering column trim cover. Refer to Steering Column Trim Covers Replacement in Steering Wheel and Column.
4. Install the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .