For 1990-2009 cars

# Service Information Regarding Redesigned Wiper Linkage and New Service Procedures

Subject: | Service Information Regarding Redesigned Wiper Linkage and New Service Procedures.

Models: | 2000 - 2003 L-Series vehicles

### Purpose

The purpose of this bulletin is to notify you about a redesigned wiper linkage and to provide new service procedures regarding linkage and motor replacement. A redesigned front wiper linkage is being used on all 2003 model year L-Series vehicles. This redesign includes a change from 12 mm ball and socket attachments between the motor and the linkage to a 14 mm ball and socket attachment between the motor and linkage. All Linkage service parts P/N 22699213 will be the 2003 design and can be used to back service 2000 thru 2003 models. The replacement linkage will include an updated motor crank arm with a 14 mm ball stud, a new washer and attachment nut. The redesign will require the new motor crank arm be attached to the existing motor when replacing the front wiper linkage on 2000 thru 2002 L-Series vehicles.

In addition the replacement front wiper motor service part P/N 22699805 will not be provided with a crank arm. This will require the technician to transfer the crank arm from the original motor to the replacement motor on all 2000 thru 2003 L-Series vehicles.

Follow the service procedures in this bulletin when replacing a front wiper motor, or front wiper linkage. For installation of the crank arm to the motor, timing of the motor, and crank arm to the front linkage, refer to the "Wiper/Washer" section of the applicable year Body/Electrical Volume II Service Manual for wiper motor and linkage removal.

### Wiper Motor Replacement 2000 - 2002 Model Years

1. Remove wiper motor crank arm from wiper motor.
2. Remove three wiper motor fasteners and remove wiper motor from linkage.
3. Install new wiper motor on linkage and install fasteners.

Tighten
Tighten to wiper motor-to-frame fasteners to 5 N·m (44 lb in).

Important: Steps 4-6 are required to ensure the wiper motor and crank arm are properly timed to the linkage.

4. Connect the wiper motor into the vehicle wiper electrical harness.
5. With the key on, cycle the wiper switch to the "Low Speed" position, and then back to "Park". This will ensure the wiper motor is in the "Park" position before installing the wiper motor crank arm.
6. Install wiper motor crank arm, aligning it in between the alignment marks on the linkage mounting plate.
7. Install crank arm washer and nut.

Tighten
Tighten the wiper motor crank arm nut to 15 - 20 N·m (11 - 15 lb ft).

8. Install linkage connecting wiper arm to wiper motor crank arm ball stud.
9. Refer to the "Wiper/Washer" section of the applicable year Body/Electrical Volume II Service Manual for installation of the linkage and motor to vehicle.

### Linkage Replacement 2000 - 2002 Model Years

1. Remove wiper motor crank arm from motor and discard.
2. Remove three wiper motor fasteners and remove wiper motor from linkage.
3. Install wiper motor on new linkage and install fasteners.

Tighten
Tighten the wiper motor-to-frame fasteners to 5 N·m (44 lb in).

Important: Steps 4-6 are required to ensure wiper motor and crank arm are properly timed to linkage.

4. With the key on, cycle the wiper switch to the "Low Speed" position, and then back to "Park". This will ensure the motor is in the "Park" position before installing wiper motor crank arm.
5. Install the 14 mm wiper motor crank arm (provided with the replacement linkage), aligning it in between the alignment marks on the linkage mounting plate.
6. Install crank arm washer and nut.

Tighten
Tighten the wiper motor crank arm nut to 15 - 20 N·m (11 - 15 lb ft).

7. Install linkage connecting arm-to-wiper motor crank arm ball stud.
8. Refer to the "Wiper/Washer" section of the applicable year Body/Electrical Volume II Service Manual for installation of the linkage and motor to vehicle.

### Wiper Motor Replacement 2003 Model Year

1. Remove wiper motor crank arm from wiper motor and save for reinstallation.
2. Remove three wiper motor fasteners and remove wiper motor from linkage.
3. Install new wiper motor on linkage and install fasteners.

Tighten
Tighten the wiper motor-to-frame fasteners to 5 N·m (5 lb in).

Important: Steps 4-6 are required to ensure the wiper motor and crank arm are properly timed to the linkage.

4. Connect the wiper motor into the vehicle wiper electrical harness.
5. With the key on, cycle the wiper switch to the "Low Speed" position, and then back to "Park". This will ensure the wiper motor is in the "Park" position before installing the wiper motor crank arm.
6. Install wiper motor crank arm, aligning it in between the alignment marks on the linkage mounting plate.
7. Install crank arm washer and nut.

Tighten
Tighten the wiper motor crank arm nut to 15 - 20 N·m (11 - 15 lb ft).

8. Install linkage connecting wiper arm to wiper motor crank arm ball stud.
9. Refer to the "Wiper/Washer" section of the applicable year Body/Electrical Volume II Service Manual for installation of the linkage and motor to vehicle.

### Linkage Replacement 2003 Model Year

1. Remove wiper motor crank arm from motor.
2. Remove three wiper motor fasteners and remove wiper motor from linkage.
3. Install wiper motor on linkage and install fasteners.

Tighten
Tighten the wiper motor-to-frame fasteners to 5 N·m (5 lb in).

Important: Steps 4-6 are required to ensure the wiper motor and crank arm are properly timed to the linkage.

4. Plug wiper motor into vehicle wiper electrical harness.
5. With the key on, cycle the wiper switch to the "Low Speed" position, and then back to "Park". This will ensure the motor is in the "Park" position before installing wiper motor crank arm.
6. Install the 14mm wiper motor crank arm (provided with the replacement linkage), aligning it in between the alignment marks on the linkage mounting plate.
7. Install crank arm washer and nut.

Tighten
Tighten the wiper motor crank arm nut to 15 - 20 N·m (11 - 15 lb ft).

8. Install linkage connecting arm-to-wiper motor crank arm ball stud.
9. Refer to the "Wiper/Washer" section of the applicable year Body/Electrical Volume II Service Manual for installation of the linkage and motor to vehicle.

### Parts Requirements

Part Number | Description
--- | ---
22699213 | Frame ASM-WSW Trans
22699805 | Motor ASM-WSW

### Claim Information

To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System for B1789 (Link, Wiper Windshield (One or Both) - R or Replace) or N3520 (Motor, Wiper, Windshield - Replace), refer to the appropriate Electronic Labor Time Guide for the correct Labor Operation Code and Time.